2350 2400 2450 2500 2550 2600 2650

7850

7900

7950

8000

98

8478

Centerlines Picked 3 Times, Then Uniformly Interpolated; Results Smoothed; then Half-Meanders IDd using Inflection Points Half-Meanders with Sinuosity <1.1 not measured (red). Channel Centerline ID:47

distance x (m) distance y (m)

-2269

-2268

-2267

-2266

-2265

-2264

-2263

-2262

-2261