-2500 -2400 -2300 -2200 -2100 -2000 0 20 40 60 80 100 120 140 Raw elevation, color is log2(quality), comparison of deprecated (circles) to preferred (errorbars) dotting strategies

Raw elevation

Channel width