100 150 200 400 600 800 -80 -60 -40 -20 0 20 40 60 80 100 120

meander wavelength (m)

Elevation relative to interpolated F1/F2 contact (m) quadratic correction, Half-meander wavelength versus corrected elevation Color corresponds to E position (km)